**Apalachicola (APA) NERR Meteorological Metadata**

**January 2018 – December 2018**

**Latest Update: January 23, 2020**

**I.Data Set & Research Descriptors**

**1)Principal investigator & contact persons:**

Jason Garwood, Research Coordinator

[Jason.garwood@dep.state.fl.us](mailto:Jason.garwood@dep.state.fl.us)

850-670-7705

Ethan Bourque, Environmental Specialist

[Ethan.bourque@dep.state.fl.us](mailto:Ethan.bourque@dep.state.fl.us)

850-670-7722

Lauren Levi, Environmental Specialist

[Lauren.levi@dep.state.fl.us](mailto:Lauren.levi@dep.state.fl.us)

850-670-7710

Megan Lamb, Environmental Specialist

[Megan.lamb@dep.state.fl.us](mailto:Megan.lamb@dep.state.fl.us)

850-670-7709

Florida Department of Environmental Protection

Apalachicola National Estuarine Research Reserve

108 Island Drive

Eastpoint, FL 32328

**2)Entry verification:**

Data are uploaded from the CR1000/CR1000X data logger to a Personal Computer (IBM compatible). Files are exported from LoggerNet in a comma-delimited format and uploaded to the CDMO where they undergo automated primary QAQC and become part of the CDMO’s online provisional database. During primary QAQC, data are flagged if they are missing or out of sensor range. The edited file is then returned to the Reserve where it is opened in Microsoft Excel and processed using the CDMO’s NERRQAQC Excel macro. The macro inserts station codes, creates metadata worksheets for flagged data and summary statistics, and graphs the data for review. It allows the user to apply QAQC flags and codes to the data, append files, and export the resulting data file to the CDMO for tertiary QAQC and assimilation into the CDMO’s authoritative online database. For more information on QAQC flags and QAQC codes, see Sections 11 and 12.

Ethan Bourque is responsible for all Meteorological data management with assistance from Jason Garwood.

**3)Research objectives:**

The objective of this research is to monitor meteorological data on a long-term basis. Data collected from the East Bay weather station complement those data taken from the East Bay water quality station. Data are also used in the analysis of other datalogger data collected at Cat Point, Dry Bar, Pilots Cove, and Little St. Marks. Weather station data will also be integrated with monitoring the Reserve is performing as a Sentinel Site for climate change. Positioning the weather station in East Bay allows the Reserve to monitor changes in rainfall, photosynthetically active radiation, temperature, and other weather parameters influencing the water quality of East Bay as well as climate change sentinel sites located in East Bay marshes. East Bay drains the Tate's Hell Swamp area, which was altered in the late 1960's and early 1970's by timber companies. An EPA grant allowed the Northwest Florida Water Management District to begin restoration of the site in 1995 to reduce non-point source runoff. East Bay is also an important nursery area for numerous fish and invertebrate species within Apalachicola Bay.

**4)Research methods:**

Data Collection (CR1000/CR1000X):

The 15 minute Data are collected in the following formats for the CR1000X:

Averages from 5-second data:

Air Temperature (°C), Relative Humidity (%), Barometric Pressure (mb), Wind Speed (m/s), Wind Direction (degrees), Battery Voltage (volts)

Maximum and Minimum Air Temperature (°C) and their times from 5-second data (these data are available from the Reserve)

Maximum Wind Speed (m/s) and time from 5-second data

Wind Direction Standard Deviation (degrees)

Totals:

Precipitation (mm), PAR (millimoles m-2), and Cumulative Precipitation (mm) (Cumulative precipitation is no longer available via export from the CDMO. Please contact the Reserve or the CDMO for more information or to obtain these data.)

Sensor Calibration QA/QC:

Sensors are calibrated either yearly or every 2 years according to the maintenance schedule dictated by the NERR System Wide Monitoring Program SOPs. The sensors and their wires are inspected monthly to make sure that they are clean, moving freely, and undamaged. The arm of the wind sensor is checked monthly to assure that it is aligned to true north.

Recommended calibration frequency for the MET station sensors:

- Temperature/Humidity- yearly recalibration

- Rain Gauge- yearly recalibration

- Wind Speed/Direction- every 2 years recalibration for the RM Young 5103 sensor

- Barometric Pressure- every 2 years recalibration

- PAR- every 2 years recalibration

- CR1000X- every 5 years (required beginning 2014, one year initial grace period)

Data Storage/Interface with LoggerNet:

A Laptop is used to interface between the CR1000 and the LoggerNet software supplied by Campbell Scientific. Data is downloaded monthly and at the time of the download, a handheld Kestrel 4000 is used to measure weather conditions and compare them to the measurements of the sensors on the weather station. A neighboring weather station operated by Florida Department of Environmental Protection, Division of State Lands, is used for further comparison when necessary.

Telemetry:

Campbell Scientific data telemetry equipment was installed at the East Bay weather station on 06/22/2006 and transmits data to the NOAA GOES satellite, NESDIS ID #3B01C09E. The transmissions are scheduled hourly and contain four (4) data sets reflecting fifteen minute data sampling intervals. Upon receipt by the CDMO, the data undergoes the same automated primary QAQC process detailed in Section 2 above. The “real-time” telemetry data become part of the provisional dataset until undergoing secondary and tertiary QAQC and assimilation in the CDMO’s authoritative online database. Provisional and authoritative data are available at [http://cdmo.baruch.sc.edu](http://cdmo.baruch.sc.edu/).

Data are collected in Eastern Standard Time (EST) for the entire year.

**5)Site location and character:**

The Apalachicola National Estuarine Research Reserve is located in the northwestern part of Florida, generally called the panhandle. It is located adjacent to the City of Apalachicola, and encompasses most of the Apalachicola Bay system, including 52 miles of the lower Apalachicola River. Passes, both natural and manmade, connect Apalachicola Bay to the northeastern Gulf of Mexico. The sampling site is located in the upper reaches of East Bay. East Bay is separated from Apalachicola Bay by two bridges and a causeway and is located to the north of Apalachicola Bay proper. The bay is 8.2 km long, has an average depth of approximately 1.0 m MHW, and an average width of 1.8 km. The tides in East Bay are mixed and range from 0.3 m to 1.0 m (average 0.5 m).

The weather station is located at latitude 29 47' 27.24 N and longitude 84 53' 0.24 W. This site is less than 0.5 nautical miles west of the East Bay water quality station. The site is located near the tip of a peninsula, which separates Blount's Bay from West Bayou. The peninsula is dominated by marsh vegetation (mainly *Juncus roemerianus*). There is a cabbage palm hammock along the southeastern shoreline of the peninsula. The dominant upland habitat is primarily pineland forest to the northwest, which includes slash pine, saw palmetto, and sand pine. In accordance with NERR SWMP and CDMO requirements the weather station wind and PAR sensors are mounted at the top of a 3-meter tower. The temperature/relative humidity sensor and barometric pressure sensor (inside the CR1000 enclosure) are mounted on the tower at 1.5 meters. The tower is mounted on a 2 meter platform. The tipping bucket rain gauge is mounted on a 1 meter platform approximately 4 meters from the weather station platform. There is nothing nearby to shade the tower and the nearest wind block is the edge of the pine forest about 1 kilometer north to northwest of the station.

SWMP Station Timeline:

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Station Code | Station Name | SWMP Status | Location | Active Dates | Reason Decommissioned | Notes |
| APAEBMET | East Bay | P | 29°47'27.24"N 84°53'0.24" W | 01/01/2001 - | NA | NA |

**6)Data collection period:**

The Apalachicola weather monitoring station was erected on August 27, 1999 and began monitoring on September 3, 1999. The data submitted with this report encompasses data collected from 00:00 January 1, 2018 through 15:45 October 22, 2018.

|  |  |  |
| --- | --- | --- |
| **Raw File Name** | **Start Date/Time** | **End Date/Time** |
| apaebmet120817 | 12/08/2017 10:15 | 01/22/2018 09:15 |
| apaebmet012218 | 01/22/2018 09:30 | 02/07/2018 10:15 |
| apaebmet020718 | 02/07/2018 10:30 | 03/07/2018 09:00 |
| apaebmet030718 | 03/07/2018 09:15 | 03/24/2018 12:30 |
| apaebmet040218 | 04/02/2018 07:45 | 05/04/2018 07:30 |
| apaebmet050418 | 05/04/2018 07:45 | 05/22/2018 03:45 |
| apaebmet052318 | 05/23/2018 07:15 | 06/06/2018 09:15 |
| apaebmet0606718 | 06/06/2018 07:00 | 06/22/2018 06:45 |
| apaebmet062218 | 06/22/2018 07:45 | 07/03/2018 08:15 |
| apaebmet070318 | 07/03/2018 08:30 | 08/08/2018 08:45 |
| Apaebmet080818 | 08/08/2018 09:00 | 09/11/2018 08:45 |
| Apaebmet091118 | 09/11/2018 09:00 | 10/22/2018 15:45 |

**7)Distribution:**

NOAA retains the right to analyze, synthesize and publish summaries of the NERRS System-wide Monitoring Program data.  The NERRS retains the right to be fully credited for having collected and process the data.  Following academic courtesy standards, the NERR site where the data were collected should be contacted and fully acknowledged in any subsequent publications in which any part of the data are used.  The data set enclosed within this package/transmission is only as good as the quality assurance and quality control procedures outlined by the enclosed metadata reporting statement.  The user bears all responsibility for its subsequent use/misuse in any further analyses or comparisons.  The Federal government does not assume liability to the Recipient or third persons, nor will the Federal government reimburse or indemnify the Recipient for its liability due to any losses resulting in any way from the use of this data.

Requested citation format:

NOAA National Estuarine Research Reserve System (NERRS). System-wide Monitoring Program. Data accessed from the NOAA NERRS Centralized Data Management Office website: <http://www.nerrsdata.org/>; *accessed* 12 October 2018.

NERR meteorological data and metadata can be obtained from the Research Coordinator at the individual NERR site (please see Principal Investigators and Contact Persons), from the Data Manager at the Centralized Data Management Office (please see personnel directory under the general information link on the CDMO home page) and online at the CDMO home page [www.nerrsdata.org](http://www.nerrsdata.org).  Data are available in comma delimited format.

**8)Associated researchers and projects:**

Harper, J., Wren, K., Jones, D., Garwood, J., Garland, H., Snyder, C., Levi, L., Bourque, E./ NERRS Sentinel Sites Program for Understanding Climate Change Impacts on Estuaries

Edmiston, H.L., Farhny, S., Lamb, M., Levi, L., Wanat, J., Avant, J., Selly, N. Apalachicola National Estuarine Research Reserve. Tropical Storm and Hurricane Impacts on a Gulf Coast Estuary: Apalachicola Bay, Florida USA.

Garwood, J., Harper, J., Levi, L., Lamb, M., Jones, D., Garland, H., Bourque, E., Yuan, W., Christopher, M., Cox, N. Apalachicola National Estuarine Research Reserve. Distribution and density of fishes and benthic invertebrates in Apalachicola Bay.

Harper, J., Levi, L., Jones, D., Lamb, M., Garwood, J., Garland, H., Bourque, E. Apalachicola National Estuarine Research Reserve. System-Wide Monitoring Program (SWMP) for water quality, weather, nutrients & chlorophyll A, and submerged aquatic vegetation monitoring in Apalachicola Bay.

Gilhring, T. Florida State University. The role of oligohaline marshes as a source or sink of nitrogen to the Apalachicola Bay.

Peterson, R. Florida State University. Origin and fate of suspended particulates in the Apalachicola River: Impact on Apalachicola Bay.

Putland, J. Florida State University Department of Oceanography. NOAA Graduate Research Fellowship. Planktonic food web variations related to salinity and nutrient patterns in Apalachicola Bay.

Wang, H., Huang, W., Harwell, M., Edmiston, H.L., Johnson, E., Hsieh, P., Milla, K., Christensen, J., Stewart, J., Liu, X. 2008. Modeling oyster growth rate by coupling oyster population and hydrodynamic models for Apalachicola Bay, Florida, USA. Ecological Modeling 211:77-89.

Viveros, P. NOAA Graduate Research Fellowship, Phytoplankton composition and abundance in relation to salinity, nutrient and light gradients in the Apalachicola National Estuarine Research Reserve.

Anderson, C. Auburn University, School of Forestry and Wildlife Sciences. Response of coastal riverine wetlands to water allocations in an urbanizing watershed.

Smith, S. Florida A&M University post-doctoral research associate, ECSC/Environmental Sciences Institute, Drought, Reduced River Flow and Sea Level Rise: Exploring Climate Impacts on Carbon and Nitrogen Cycling in the Apalachicola Bay System.

Hagen, S., DeLorme, D., Walters, L., Wang, D., Weishampel, J., Yeh, G., Huang, W., Slinn, D., Morris, J. Ecological Effects of Sea Level Rise.

As part of the SWMP long-term monitoring program, APANERR also monitors 15-minute water quality along with monthly grab samples and diel sampling for nutrient data which may be correlated with this meteorological dataset. These data are available at [www.nerrsdata.org](http://www.nerrsdata.org).

**II.Physical Structure Descriptors**

**9)Sensor Specifications:**

Parameter: Temperature

Units: Celsius

Sensor type: 100 ohm platinum resistance temperature detector (PRT)

Model #: Rotronic HC2-S3 Temperature and Relative Humidity Probe

Operating Temperature: -40oC to +60oC

Range: -40oC to +60oC

Accuracy: +/- 0.1oC (@ 23oC

S/N: 0061247971

Date of calibration: 03/23/2016

Dates of sensor use: 03/23/2016 – 03/08/2017

S/N: 0061212271

Date of calibration: 01/27/2017

Dates of sensor use: 03/08/2017 – 03/07/2018

S/N: 20076010

Date of calibration: 03/07/2018

Dates of sensor use: 03/07/2018 – current as of 10/22/2018

Parameter: Relative Humidity

Units: Percent

Sensor type: ROTRONIC® Hygromer IN-1

Model #: Rotronic HC2-S3 Temperature and Relative Humidity Probe

Range: 0-100% non-condensing

Accuracy at 23°C:  +/- 0.8% RH with standard configuration settings

Temperature dependence of RH measurement +/- 3% (-40 to 60C)

S/N: 0061212271

Date of calibration: 01/27/2017

Dates of sensor use: 03/08/2017 – 03/07/2018

S/N: 0061247971

Date of calibration: 03/23/2016

Dates of sensor use: 03/23/2016 – 03/08/2017

S/N: 20076010

Date of calibration: 03/07/2018

Dates of sensor use: 03/07/2018 – current as of 10/22/2018

Parameter: Barometric Pressure

Units: millibars (mb)

Sensor type: Vaisala Barocap © silicon capacitive pressure sensor

Model #: PTB110

Operating Range: Pressure: 600 to 1060 mb; Temperature: -40°C to +60°C;

Humidity: non-condensing

Accuracy: ± 0.5 mb @ 20°C; +/- 2 mb @ 0°C to 40°C; +/- 4 mb @ -20°C to 45°C; +/- 6 mb @ -40°C to 60°C

Stability: ± 0.1 mb per year

S/N: K0220004

Date of calibration: 01/13/2014

Dates of sensor use: 02/23/2016 – 01/22/2018

S/N: N4130442

Date of calibration: 01/22/2018

Dates of sensor use: 01/22/2018 – current as of 10/22/2018

Parameter: Wind speed

Units: meter per second (m/s)

Sensor type: 18 cm diameter 4-blade helicoids propeller molded of polypropylene

Model #: R.M. Young 05103 Wind Monitor

Range: 0-60 m/s (134 mph); gust survival 100 m/s (220 mph)

Accuracy: +/- 0.3 m/s

S/N: WM127200

Date of calibration: 03/03/2016

Dates of sensor use: 04/11/2016– 04/04/2017

S/N: WM131274

Date of calibration: 01/31/2017

Dates of sensor use: 04/04/2017– current as of 10/22/2018

Parameter: Wind direction

Units: degrees

Sensor type: balanced vane, 38 cm turning radius

Model #: R.M. Young 05103 Wind Monitor

Range: 360° mechanical, 355° electrical (5° open)

Accuracy: +/- 3 degrees

S/N: WM127200

Date of calibration: 03/03/2016

Dates of sensor use: 04/11/2016– 04/04/2017

S/N: WM131274

Date of calibration: 01/31/2017

Dates of sensor use: 04/04/2017– current as of 10/22/2018

\*\*Note\*\* The arm of the wind sensor is checked monthly to ensure that it remains aligned to true north.

Parameter: Photosynthetically Active Radiation

Units: millimoles m-2 (total flux)

Sensor type: Un-amplified quantum sensor

Model #: SQ-110 Apogee

Light spectrum waveband: 410 to 655 nm

Temperature dependence: 0.06 ± 0.06% per °C

Stability: <±2% change over 1 yr

Operating Temperature: -40°C to 70°C; Humidity: 0 to 100%

Sensitivity: 0.2 mV per µmole m-2 s-1

Multiplier: 0.025

Field of view: 180°

S/N: 19559

Date of calibration: 12/01/2015

Dates of sensor use: 04/11/2016 – 05/25/2017

S/N: 22808

Date of calibration: 05/25/2017

Dates of sensor use: 05/25/2017 – current as of 10/22/2018

Parameter: Precipitation

Units: millimeters

Sensor type: Tipping Bucket Rain Gauge

Model #: TR525 USW

Funnel diameter: 8.0 inches

Rainfall per tip: 0.01 inch

Operating range: Temperature: 0° to 50°C; Humidity: 0 to 100%

Accuracy: +/- 1.0% up to 1 in./hr; +0, -3% from 1 to 2 in./hr; +0, -5% from 2 to 3 in./hr

S/N: 59238-314

Date of calibration: 03/08/2017

Dates sensor use: 05/14/2014 –05/04/2018

Units: millimeters

Sensor type: Tipping Bucket Rain Gauge

Model #: TR525 USW

Funnel diameter: 6.0 inches

Rainfall per tip: 0.01 inch

Operating range: Temperature: 0° to 50°C; Humidity: 0 to 100%

Accuracy: +/- 1.0% up to 1 in./hr; +0, -3% from 1 to 2 in./hr; +0, -5% from 2 to 3 in./hr

S/N: 74048

Date of calibration: 05/04/2018

Dates sensor use: 05/04/2018 – current as of 10/22/2018

Compact Flash Module

Model #: CFM100

Storage capacity: 64 MB

Operating range: Temperature: -35° to +65°C

Memory type: user selectable for either ring style (default) or fill and drop.

Power requirements: 12 V supplied through CR1000 peripheral port

In Use Dates are from 08/07/2006 – 06/22/2018

CR1000 Datalogger

The CR1000 has two MB Flash EEPROM that are used to store the Operating System. Another 128 K Flash is used to store configuration settings. A minimum of 2 MB SRAM is (4 MB optional) is available for program storage (16K), operating system use, and data storage. Additional storage is available by using a compact flash card in the optional CFM100 Compact Flash Module.

CR1000

S/N: 56121

Calibration: 05/31/2013

Installed: 06/14/2013

Removed: 05/04/2018

S/N: 005091

Calibration: 01/16/2018

Installed: 05/04/2018

Removed: 06/22/2018

CR1000X

The CR1000X has 4 MB of battery backed SRAM that is used for CPU usage and Final Storage. An additional 4 MB of SRAM is used for program storage, configuration settings, and operating system storage. Another 72 MB of Flash memory is used for data storage. Additional storage is available by using a microSD (up to 16GB) flash card using the integrated reader.

CR1000X

S/N: 3360

Calibrated: 05/11/2018

Installed: 06/22/2018

Removed: 11/09/2018

CR1000 Firmware Version 24 in use from 08:45 10/12/2012 – 14:15 02/14/2014

CR1000 Firmware Version 27 in use from 14:30 02/14/2014 – 07:30 05/04/2018

CR1000 Firmware Version 32.02 in use from 08:00 05/04/2018 - 08:00 06/22/2018

CR1000X Firmware Version 1.02 in use from 08:00 06/22/2018 – current

CR1000 Program Version:

apaebmet\_5.6\_072513 in use 9:15 07/26/2013 – 12:00 01/23/2014.

apaebmet\_5.6\_122013 in use 12:15 01/23/2014 – 10:15 01/14/2015

apaebmet\_5.6\_010715 in use 10:30 01/14/2015 – 10:00 02/16/2016

apaebmet\_5.6\_020816 in use 10:15 02/16/2016 – 10:00 04/11/2016

apaebmet\_5.6\_032316 in use 10:30 04/11/2016 – 08:00 06/22/2018

apaebmet\_CR1000X\_5.6\_061518 08:30 06/22/2018 – current as of 10/22/2018

**10)Coded variable indicator and variable code definitions:**

Sampling station: Sampling site code: Station code:

East Bay EB apaebmet

**11)QAQC flag definitions:**

QAQC flags provide documentation of the data and are applied to individual data points by insertion into the parameter’s associated flag column (header preceded by an F\_). During primary automated QAQC (performed by the CDMO), -5, -4, and -2 flags are applied automatically to indicate data that is above or below sensor range or missing. All remaining data are then flagged 0, as passing initial QAQC checks. During secondary and tertiary QAQC 1, -3, and 5 flags may be used to note data as suspect, rejected due to QAQC, or corrected.

-5 Outside High Sensor Range

-4 Outside Low Sensor Range

-3 Data Rejected due to QAQC

-2 Missing Data

-1 Optional SWMP supported parameter

0 Passed Initial QAQC Checks

1 Suspect Data

2 *Open - reserved for later flag*

3 *Open - reserved for later flag*

4 Historical Data: Pre-Auto QAQC

5 Corrected Data

**12)QAQC code definitions:**

QAQC codes are used in conjunction with QAQC flags to provide further documentation of the data and are also applied by insertion into the associated flag column. There are three (3) different code categories, general, sensor, and comment. General errors document general problems with the CR1000, sensor errors are sensor specific, and comment codes are used to further document conditions or a problem with the data. Only one general or sensor error and one comment code can be applied to a particular data point, but some comment codes (marked with an \* below) can be applied to the entire record in the F\_Record column.

General Errors

GIM Instrument malfunction

GIT Instrument recording error, recovered telemetry data

GMC No instrument deployed due to maintenance/calibration

GMT Instrument maintenance

GPD Power down

GPF Power failure / low battery

GPR Program reload

GQR Data rejected due to QA/QC checks

GSM See metadata

Sensor Errors

SDG Suspect due to sensor diagnostics

SIC Incorrect calibration constant, multiplier or offset

SIW Incorrect wiring

SMT Sensor maintenance

SNV Negative value

SOC Out of calibration

SQR Data rejected due to QAQC checks

SSD Sensor drift

SSN Not a number / unknown value

SSM Sensor malfunction

SSR Sensor removed

Comments

CAF Acceptable calibration/accuracy error of sensor

CCU Cause unknown

CDF Data appear to fit conditions

CML Snow melt from previous snowfall event

CRE\* Significant rain event

CSM\* See metadata

CVT\* Possible vandalism/tampering

CWE\* Significant weather event

**13) Other Remarks/ Notes**

Data are missing due to equipment or associated specific sensors not being deployed, equipment failure, time of maintenance or calibration of equipment, or repair/replacement of a sampling station platform. Any NANs in the dataset stand for “not a number” and are the result of low power, disconnected wires, or out of range readings. If additional information on missing data is needed, contact the Research Coordinator at the reserve submitting the data.

Small negative PAR values are within range of the LI-COR sensor and are due to normal errors in the sensor and the CR1000 Datalogger. The Maximum signal noise error for the LI-COR sensor is +/- 2.214 mmoles/m2 over a 15 minute interval. These values are automatically flagged and coded as <1> (CAF).

Relative Humidity data greater than 100 are within range of the sensor accuracy of +/-3% and are flagged and coded as suspect, <1> (CAF). Values greater than 103 are rejected <-3>.

Data recorded for all parameters (with the exception of cumulative precipitation) at the midnight timestamp (00:00) are the 15 minute averages and totals for the 23:45-23:59 time period of the previous day. Cumulative precipitation data at the midnight timestamp (00:00) are the sum of raw (unrounded) precipitation data from 00:00 to 23:59 of the previous day. Summing each individual 15-minute total precipitation value from the same period will result in small differences from cumulative precipitation due to rounding. It is especially important to note how data at the midnight timestamp are recorded when using January 1st and December 31st data. **Note: Cumulative precipitation is no longer available via export from the CDMO. Please contact the Reserve or the CDMO for more information or to obtain these data.**

Apogee nighttime PAR values greater than 0.0 mmoles m-2 are flagged and coded as <1> (CSM), indicating that users should be aware of possible data inconsistencies. Nighttime periods were determined using sunrise-sunset times obtained from <http://www.sunrisesunset.com>.

01/20/2018 12:15 data are rejected due to a low minimum air temperature value (-39.3) (minimum and maximum air temperature are available from the reserve). Relative humidity is rejected since those readings are temperature dependent. Air temperature and relative humidity on 04/09/2018 05:15, 04/16/2018 12:00, 05/15/2018 03:45, 09/14/2018 15:00, and 16:30 are also rejected due to low minimum air temperature readings.

01/22/2018 09:30 through 02/07/2018 10:30 all barometric pressure data is rejected due to the internal jumper setting. Jumper setting was corrected to continuous on 02/07/2018 at 10:30.

03/07/2018 09:00 – 09:15 air temperature and relative humidity are both rejected due to maintenance to swap the sensor.

03/24/2018 12:45 through 04/02/2018 07:30 all data are missing due to station shut down. Reason for shutdown is unknown. All parameters 04/02/2018 07:45 rejected due to most likely not being a full 15 minutes of 5-second data following the station shut down.

05/04/2018 07:45 through 08:00 to replace CR1000 datalogger SN: 56121 (OUT) SN: 5091 (IN). All parameters rejected due to maintenance.

05/04/2018 07:45 through 08:30 replaced rain gauge, reject Total Precipitation

05/04/2018 07:45 through 12:00 reject Cum Precipitation values cause by installation of new rain gauge

05/04/2018 14:15 all parameters rejected due to most likely not being a full 15 minutes of 5-second data following a brief period when the CR1000 was not recording.

05/16/2018 08:00 through 05/21/2018 11:30 and 05/22/2018 04:00 through 05/23/2018 data missing due to CR1000 datalogger not having enough memory to run programming, F\_Record coded {CSM}. All parameters rejected at 05/21/2018 11:45 and 05/23/2018 07:15 due to most likely not being a full 15 minutes of 5-second readings.

05/21/2018 11:45 – 5/22/2018 00:00 cumulative precipitation data are considered suspect. Since the CR1000 had stopped recording we do not know if those rainfall occurred on 05/21/2018 or if they were stored on the data logger from rainfall on 5/16/2018.

05/23/2018 07:30 through 06/22/2018 06:45 all data suspect due to reinstallation of uncalibrated logger SN: 56121 to replace the logger SN: 5091 that couldn’t support programming and was not collecting data, this was done with CDMO advisement

05/26/2018 13:15 – 05/30/2018 08:00 Hurricane Alberto; included in suspect data mentioned above

05/23/2018 20:30 – 05/04/2018 05:00, 05/24/2018 20:15 -05/25/2018 05:15, 05/25/2018 20:15 – 05/26/2018 05:00, 05/26/2018 20:15 – 05/27/2018 05:15, 05/27/2018 20:15 – 05/28/2018 05:15, 05/28/2018 20:15 – 05/29/2018 05:15, 05/29/2018 20:15 – 05/30/2018 05:15, 05/30/2018 20:15 -05/31/2018 05:00, 05/31/2018 20:15 – 06/01/2018 05:00, 06/01/2018 20:15 – 06/02/2018 05:15, 06/02/2018 20:15 – 06/03/2018 05:15, 06/03/2018 20:15 - 06/04/2018 05:15, 06/04/2018 20:15 – 06/05/2018 05:15, 06/05/2018 20:15 – 06/06/2018 05:15, 20:15 – 06/07/2018 05:15, 06/07/2018 20:15 – 06/08/2018 05:00, 06/08/2018 20:15 – 06/09/2018 05:15, 06/09/2018 20:15 – 06/10/2018 05:15, 06/10/2018 20:15 – 06/11/2018 05:15, 06/11/2018 20:15 – 06/12/2018 05:00, 06/12/2018 20:30 – 06/13/2018 05:15, 06/13/2018 20:30 – 06/14/2018 05:00, 06/14/2018 20:30 – 06/15/2018 05:15, 06/15/2018 20:15 – 06/16/2018 05:15, 06/16/2018 20:30 - 06/17/2018 05:15, 06/17/2018 20:15 – 06/18/2018 5:15, 06/18/2018 20:30 – 06/19/2018 05:15, 06/19/2018 20:15 – 06/20/2018 05:15, 06/20/2018 20:15 -06/21/2018 05:15, 06/21/2018 20:30 – 06/22/2018 05:15 reject elevated nighttime PAR data

06/03/2018 07:00 reject Temp RH values, negative minimum

06/22/2018 07:00 – 07:30 Data missing due to logger swap CR1000X SN: 3360 (IN) CR1000 SN: 56121 (OUT). Data at 07:45 are rejected due to most likely not being a full 15 minutes of 5-second data following the logger swap.

10/08/2018 12:00 – 10/11/2018 08:30 Hurricane Michael, landfall 11:00-12:00 on 10/10/2018. F\_Record coded with CSM for duration of storm.

Max Wind Speed readings 10/10/2018 11:45 – 12:30 and 13:00 were initially flagged <-5> during the automatic QA/QC process which normally indicate that a reading is outside the range of the sensor. In this case however, the flagging indicated that a wind reading was high enough that the data should be checked to ensure the sensor is functioning correctly. These data are not considered suspect as Hurricane Michael was making landfall.

10/10/2018 10:00 – 10/22/2018 13:00, 13:30 - 14:00, 14:30 – 15:45 Suspect CumPrcp and Total Precip hurricane storm surge over height of rain gauge and left dirt on tipping bucket

10/22/2018 16:00 – 12/31/2018 23:45 data missing due to station damage from Hurricane Michael